The Frontier Design Tranzport is supported in native mode.

--- track selection ---

TRACK <        : to previous mixer section.
SHIFT TRACK <  : to first section.
TRACK >        : to next mixer section.
SHIFT TRACK >  : to last section.

The data wheel can be used for track selection while one of these buttons is down.


--- track control ---

REC            : toggle track Play and Rec buttons
MUTE           : mute mixer section
SOLO           : solo mixer section 
SHIFT SOLO     : clear solo
ANY SOLO       : lights up if a mixer section is soloed.
UNDO           : editor Undo (for undoing punch-in recordings).
SHIFT UNDO     : Redo

Data Wheel     : edit current parameter (volume fader, pan knob etc.).
SHIFT Data Wheel: select parameter

  Available parameters:

  T = Transport (control Transport position). Works only if transport is stopped.
  V = Volume Fader
  P = Pan
  1 = Effect Send 1
  2 = Effect Send 2
  3 = Effect Send 3
  O = Output Selector
  M = Mouse Control (the control the mouse is on)


--- punch-in recording ---

IN             : Set current track's punch-in point
                 (make it equal to current transport position)
SHIFT In       : move to punch-in point
OUT            : Set current track's punch-out point
                 (make it equal to current transport position)
SHIFT OUT      : move to punch-out point
FOOTSWITCH     : Set current track's punch in and out points on-the-fly (equals clicking the track's editor).
PUNCH          : toggle punch in/out recording


--- alternate takes and new tracks ---

SHIFT PUNCH    : alternate take
                 (invokes the Alternate Take option from the Recording menu)
SHIFT LOOP     : add track with new file and copy all settings from current track
SHIFT PREV     : New audio track (pick one from list of audio track templates)
SHIFT NEXT     : New MIDI track (pick one from list of MIDI track templates)


--- markers ---

PREV           : to previous marker
ADD            : add marker
SHIFT ADD      : delete marker (use PREV, ADD or NEXT first)
NEXT           : to next marker


--- transport ---

<<             : Rewind
SHIFT <<       : Home
>>             : Fast Forward
SHIFT >>       : to End
STOP           : Stop
SHIFT STOP     : to last start position ("ALT - cursor left")
PLAY           : Play
SHIFT PLAY     : to next start position ("ALT - cursor right")
LOOP           : turn Cycle on/off (Start will start cycling if it's on)

REC            : "What Is?", Push another button while keeping this one down
                  to see the button's function on the display for one second.
REC LED        :  The LED lights if one or more tracks are armed for recording
                  (ie. its Rec button is red).


--- message dialogs ---

STOP           : 'Cancel' or 'No'
PLAY           : 'OK' or 'Yes'
<<             : Show previous two lines of message
SHIFT <<       : to first lines
>>             : Show next two lines of message
SHIFT >>       : to last lines


--- new file properties dialogs ---

STOP / PLAY    : 'OK'
Data Wheel     : Quality (16 or 24 bits etc.)
Track < / >    : Channels (mono or stereo)


--- display ---

Top left       : track name
Top right      : transport position indicator
                 (in seconds or bars, follows MultitrackStudio setting)
Bottom left    : level meter, equals the green and yellow sections of the
                 MultitrackStudio meters. '|' indicates 0 dB, it turns
                 into a black space if overload occured.
Bottom right   : data wheel parameter value (volume level etc.)