These HUI functions are supported:


mixer control:
8 faders
8 rotary knobs
PAN, SEND A, SEND B, SEND C, SEND D, Send E buttons to assign rotary knobs.
  Send E controls the output selector
8 MUTE and SOLO buttons
8 RECRdy buttons
8 level meters


transport:
STOP, PLAY, <<, >>, RT Z and RT END buttons
Transport Wheel
Rec button LED lights if any tracks are in record mode
Position counters
Write (automation recording)
Touch (automation touch mode)


banks:
BANK <, BANK >, CH <, CH > buttons
Shift+BANK <, BANK > jumps to first/last bank


effects:
7 rotary knobs
Rotary knob #8 is for selecting page