# Echo

Echo window

The Echo effect produces one or more echoes, depending on the Feedback control. If Feedback is set to zero, only one echo is produced. Otherwise, a decaying sequence of echoes is generated.

Delay controls the time it takes for the first echo to arrive (and the time between two consecutive echoes). The delay time is displayed in milliseconds and as note values.
Lo-cut sets the frequency below which attenuation occurs (this typically happens in tape echo units).
Hi-cut sets the frequency above which attenuation occurs (this also happens both in nature and in tape echo units).
TapeSim controls the amount of flutter and distortion.
Mix controls the level of the echoes mixed with the dry (input) signal (0% is dry only, 100% is echo only).