# Saturator

The Saturator effect adds either tube or tape-style distortion, depending on the Tube and Tape buttons. The Drive knob controls the amount of distortion. The output level is approximately equal to the input level.

### Tube

Saturator window ('Tube')

The Tube program simulates a preamp with an output transformer. The preamp mainly generates second-order harmonics, while the transformer adds lower-order odd harmonics. The Tube program enhances harmonic content, somewhat like an exciter effect.

Drive controls the signal level fed into the virtual preamp's input. The VU meter shows the average level. At 0 dB, total harmonic distortion is approximately 2%.

### Tape

Saturator window ('Tape')

The Tape program models distortion, high-frequency compression, low-frequency bump, and wow & flutter. It can be used on individual tracks to make them sound warmer. The Tape program can also be used on a full mix (i.e., in the Master section) to help tracks blend better.

Drive controls the virtual recording level. The VU meter shows the average recording level. At 0 dB VU, total harmonic distortion is approximately 1%.
LF Bump controls the low-frequency bump. Flutter controls the amount of wow & flutter.