These Mackie Control functions are supported:


--- mixer control ---

8 RecRdy buttons
8 faders
8 Mute and Solo buttons. The Solo button in the transport section clears all solo buttons.
8 rotary knobs
PAN, SEND and TRACK buttons to assign rotary knobs (TRACK controls section output selector)
8 level meters
Master fader


--- bank/channel selection ---

Bank Up and Down buttons
Channel Up and Down buttons
Shift+Bank Up/Down jumps to first/last bank


--- transport ---

<<, >>, Stop, Start Playback and Start Recording buttons
Shift+<< jumps to the beginning
Shift+>> jumps to the end
Transport Wheel
SMPTE/Beats toggles position indicator format
Rec button LED lights if any tracks are in record mode
Marker toggles marker mode, in which << and >> step through markers
Option+<< jumps to previous start position
Option+>> jumps to previous next position
Cycle toggles the Loop button
Cycle+<< sets loop start
Cycle+>> sets loop end
Drop toggles the Punch button
Write (automation recording)
Touch (automation touch mode)


--- punch-in recording ---

Select+<< sets punch-in point for this track
Select+>> sets punch-out point for this track
Select+Undo undoes editor for this track


--- effects/instruments ---

7 rotary knobs, rotary knob #8 is for selecting pages
Select+Plugin opens the first slot for this section (the Select buttons act as a modifier, just like Shift)
Plugin closes the current effect/instrument window, and opens the one on the right
Cancel closes the effect/instrument window


--- message dialogs ---

Cancel and Enter